|  |  |  |  |
| --- | --- | --- | --- |
| **Cooking Area** | **Qty.** | **U/price** | **Total** |
| **Description** |  |  |  |
| 1 | **FOUR BURNER GAS RANGE WITH OVEN, 70 CM DEPTH**- Body is made of Stainless Steel AISI 304.- Top is made of one piece of Stainless Steel AISI 304, 1.2mm thickness, which made it very easy to clean and maintained the burners isolated from dirt and wearing out.- The treated cast iron pan supports provide a heavy duty and continuous surface over the top for easier movement of the pans between burners.- Heating done through double flamed burners made of treated cast iron. Provided with flame pilot and safety device to cut gas in case of flame failure.- GN 2/1 oven internally is made of Stainless Steel AISI 304, thermostatically controlled up to 340 °C with safety device to cut out gas in case of flame failure.- Oven is also provided with special configuration cast iron base for optimum cooking performance.- Stainless Steel height adjustable feet. | **1** |  |  |
| 2 | **NEUTRAL UNIT, 60 CM** - Body entirely made of stainless steel AISI 304.- Work top made of 1.2mm polished stainless steel and reinforced by stainless steel channels.- Body is closed from three sides and provided with two hinged doors from front.- Provided with intermediate and lower shelves.- Stainless steel height adjustable feet. Technical Features: Dimensions (mm) : 600 W x 700 D x 900 H | **1** |  |  |
| 3 | **GAS FRY TOP WITH STEEL FLAT PLATE, DIM.: 80x70x90 CM** - Body is made of Stainless Steel AISI 304.- Top is made of Stainless Steel AISI 304, 1.2mm thickness.- Flat frying plate made of polished steel (Fe510D).- Heating by means of Stainless Steel burners complete with weep pilot and simmer control valve with flame failure safety device. Two independent heating zones (for double size) can be controlled separately which means that different foods can be cooked in the same time at different temperature.- Fry top is mounted on a hinged door cupboard.- Stainless Steel height adjustable feet.-Country Of Origin Jordan Technical Features: Dimensions (mm) : 800 W x 700 D x 900 H | **1** |  |  |
| 4 | **ELECTRIC CHIP DUMP** - Body is made of Stainless Steel AISI 304.- Top is made of one piece of Stainless Steel AISI 304, 1.2mm thickness.- Provided with GN 1/1 container 15cm depth. With perforated shaped false bottom to collect the oil.- Ceramic heater controlled by means of on/off switch.- Chip dump is mounted on a hinged door cupboard.- Stainless Steel height adjustable feet. Technical Features: Dimensions (mm) : 400 W x 700 D x 900 H | **1** |  |  |
| **Prep Area** |  |  |  |
| 1 | **WORK TABLE WITH BACK SPLASH, WITH LOWER SHELF, 190 CM 2**- Body entirely made of Stainless Steel AISI 304.- Work top made of 1.5mm polished Stainless Steel and reinforced by stainless steel U-shaped channels with polyurethane tapes acting as sound deadening pads.- Frame work made of 40x40mm Stainless Steel square tubes thickness of 1.2mm, all joints on the table structure fixed by welding.- Stainless Steel height adjustable feet.\* Country of origin: JORDAN Technical Features: Dimensions (mm) : 1900 W x 700 D x 900 H | **2** |  |  |
| 2 | **KARMA LARGE ELECTRIC DOUBLE TOASTER MODEL GH-813AP** - Body made of stainless steel.- Temperature control by mean of thermostat.- Grill surface made of enamelled cast iron.- Provided with internal safety thermostat.- Voltage: 220 1N\* Country of origin: CHINA Technical Features: Dimensions (mm) : 840 W x 395 D x 210 H | **1** |  |  |
| 3 | **S/S WALL SHELF, DIM.: 100x30 CM**- Body entirely made of Stainless Steel AISI 304, thickness 0.8 mm- Provided with back splash.- Country of origin : Jordan | **2** |  |  |
| 3.1 | **(Accessory) S/S WALL SHELF COLUMN 60 CM** - Made of Stainless Steel AISI 304, thickness 2.0 mm | **3** |  |  |
| 3.2 | **(Accessory) S/S WALL SHELF HOLDER 30 CM** **-** Made of Stainless Steel AISI 304, thickness 2.0 mm | **4** |  |  |
| 4 | **S/S WALL SHELF, DIM.: 90x30 CM** - Body entirely made of Stainless Steel AISI 304, thickness 0.8 mm- Provided with back splash.- Country of origin : Jordan | **2** |  |  |
| 4.1 | **(Accessory) S/S WALL SHELF COLUMN 60 CM**- Made of Stainless Steel AISI 304, thickness 2.0 mm | **3** |  |  |
| 4.2 | **(Accessory) S/S WALL SHELF HOLDER 30 CM** - Made of Stainless Steel AISI 304, thickness 2.0 mm | **4** |  |  |
| 5 | **S/S WALL SHELF, DIM.: 110x30 CM**- Body entirely made of Stainless Steel AISI 304, thickness 0.8 mm- Provided with back splash. | **2** |  |  |
| 5.1 | **(Accessory) S/S WALL SHELF COLUMN 60 CM** - Made of Stainless Steel AISI 304, thickness 2.0 mm | **4** |  |  |
| 5.2 | **(Accessory) S/S WALL SHELF HOLDER 30 CM** - Made of Stainless Steel AISI 304, thickness 2.0 mm | **4** |  |  |
| 6 | **S/S WALL SHELF, DIM.: 120x30 CM** - Body entirely made of Stainless Steel AISI 304, thickness 0.8 mm- Provided with back splash. | **1** |  |  |
| 6.1 | **(Accessory) S/S WALL SHELF HOLDER 30 CM** - Made of Stainless Steel AISI 304, thickness 2.0 mm | **2** |  |  |
| 7 | **S/S ONE DOOR VERTICAL FREEZER**- Energy efficient freezer.- Body is entirely made of Stainless Steel AISI 304 and insulated with polyurethane foam CFC-Free expansion 75mm thickness, with a density of 38 kg/m³.- Electronic temperature controlling system, automatic air defrosting system and on/off switch.- The ventilation refrigeration system positioned outside the refrigerating chamber allows an even air distribution inside the cabinet & gives extra storage space.- Evaporation tray for the condensated water.- Adjustable internal shelves in 2/1 GN size.- Doors are equipped with integrated full height stainless steel handles, easily removable magnetic gasket and self-closing mechanism.- Working temperature: (-18/-22) °C.- Capacity: 680 Ltr.- Stainless Steel height adjustable feet.- Country of Origin: JORDANTechnical Features:Dimensions (mm) : 760 W x 825 D x 2100 H | **1** |  |  |
| 8 | **S/S ONE DOOR VERTICAL REFRIGERATOR** - Energy efficient cabinet.- Body is entirely made of Stainless Steel AISI 304 and insulated with polyurethane foam CFC-Free expansion 75mm thickness, with a density of 38 kg/m³.- Electronic temperature controlling system, automatic air defrosting system and on/off switch.- The ventilation refrigeration system positioned outside the refrigerating chamber allows an even air distribution inside the cabinet & gives extra storage space.- Evaporation tray for the condensated water.- Adjustable internal shelves in 2/1 GN size.- Number of shelves: (4)- Door is equipped with integrated full height stainless steel handles, easily removable magnetic gasket and self closing mechanism.- Working temperature: (+2/+5) °C.- Capacity: 680 Ltr.- Stainless Steel height adjustable feet.- Country of Origin: JORDANTechnical Features: Dimensions (mm) : 760 W x 825 D x 2100 H | **1** |  |  |
| 9 | **HAND WASH BASIN KNEE OPERATED, DIM.: 50x35 CM** - Body entirely made of Stainless Steel AISI 304.- Naval trapezoidal wash-basin with rounded front edge, complete with 1.5" drainage pipe.- knee controlled mixer.- Wall mounted unit.\* Country of origin: ITALY Technical Features: Dimensions (mm) : 500 W x 350 D x 245 H | **1** |  |  |
| **10** | **(Accessory) SINGLE SIPHON** | **1** |  |  |
| **Self Service Line** |  |  |  |
| 1 | **CAHSHIER COUNTER (SELF SERVICE LINE) - RIGHT** - Body entirely made of Stainless Steel AISI 304 with 1.5mm top thickness.- Provided with lower and intermediate shelf.- Provided with Stainless Steel tray slide.- Stainless steel height adjustable feet. Technical Features: Dimensions (mm) : 1500 W x 1100 D x 900 H | **1** |  |  |
| 2 | **NEUTRAL UNIT (SELF SERVICE LINE)** - Body entirely made of Stainless Steel AISI 304 with 1.5mm top thickness.- Provided with lower and intermediate shelf.- Provided with Stainless Steel tray slide.- Stainless steel height adjustable feet. Technical Features: Dimensions (mm) : 1200 W x 1100 D x 900 H | **1** |  |  |
| 3 | **PASTRY REFRIGERATED DISPLAY CABINET (SELF SERVICE LINE)** - Body entirely made of Stainless Steel AISI 304 with 1.5mm top thickness.- Cabinet is provided with electronic temperature control and defrosting system.- Cabinet is provided with lower shelf.- Upper part is a cabinet made of Stainless Steel frame and fixed glass from two sides, The back of the cabinet is provided with glass sliding doors for easy refilling from the back.- The service front side is made of self-closed tilted plexi glass.- Unit provided with three glass shelves.- Cabinet is provided with Stainless Steel tray slide.- Stainless steel height adjustable feet. Technical Features: Dimensions (mm) : 1500 W x 1100 D x 1900 H | **1** |  |  |
| 4 | **S/S CORNER WORK TABLE SELF SERVECE , DIM.: 110\*110\*90 CM** - Body entirely made of Stainless Steel AISI 304.- Work top made of 1.5mm polished Stainless Steel and reinforced by stainless steel U-shaped channels with polyurethane tapes acting as sound deadening pads.- Frame work made of 40x40mm Stainless Steel square tubes thickness of1.2mm, all joints on the table structure fixed by welding.- Stainless Steel height adjustable feet.- Country of origin: Jordan - Abdin Industrial Technical Features: Dimensions (mm) : 800 W x 800 D x 900 H | **1** |  |  |
| 5 | **ELECTRIC BAIN MARIE UNIT (SELF SERVICE LINE)** - Body entirely made of Stainless Steel AISI 304 with 1.5mm top thickness.- Heated well is suitable for (4) GN 1/1, 15cm depth.- Thermostatic temperature control with indicator light.- Provided with lower shelf.- Upper curved glass shelf acting as sneeze guard.- Provided with Stainless Steel tray slide.- Stainless steel height adjustable feet.Country of origin: JordanTechnical Features:Dimensions (mm) : 1500 W x 1100 D x 900 H | **1** |  |  |
| 6 | **REFRIGERATED SALAD BAR UNIT (SELF SERVICE LINE)**- Body entirely made of Stainless Steel AISI 304 with 1.5mm top thickness.- Refrigerated well is suitable for (3) GN 1/1, 15cm depth.- Well is insulated with polyurethane foam.- Provided with electronic temperature control and defrosting system.- Provided with lower shelf.- Upper curved glass shelf acting as sneeze guard.- Provided with Stainless Steel tray slide.- Stainless steel height adjustable feet.Technical Features:Dimensions (mm) : 1200 W x 1100 D x 900 H | **1** |  |  |
| 7 | **END OF (SELF SERVICE LINE) 1** | **1** |  |  |
| 8 | **DOUBLE TUBE ELECTRIC HEATED PLATE DISPENSER** - Stainless Steel tubular plate dispenser.- Capacity: 150 plates.- Max load per tube 75 plate.- Platform safeguarded against tilting.- Spring-tension can be adjusted to the weight of the crockery.- Safety pushing handle.- Provided with four swivel castors 125mm diameter, two of which with brakes.- Four rubber bumpers.- Required plate diameter can be fixed with three adjustment rods from 230mm to 320mm.- Adjustment rods can be fixed into position.- Heated models are provided with electrical heating elements, On/Off switch and thermostat regulator (+30 to +110) °C.-Country of origin : Jordan Technical Features: Dimensions (mm) : 400 W x 850 D x 900 H | **1** |  |  |
| 9 | **S/S TRAY, BREAD AND CUTLERY UNIT (SELF SERVICE LINE), DIM.75X71X140 CM**- Body entirely made of Stainless Steel AISI 304 with 1.5mm top thickness.- Four compartments heavy-duty cutlery plastic unit.- Unit is also provided with upper shelf for bread trays.- Open tray shelf and closed cupboard from three sides.- Stainless steel height adjustable feet.\* Country of origin: Jordan Technical Features: Dimensions (mm) : 750 W x 710 D x 1400 H | **1** |  |  |
| 10 | **GLEECON GLORY INSECT KILLER MODEL GB-30L** - New and patented design- Robust housing for durable use.- High quality UV-A LED as best attraction to flying insects.- The 4 sides open outer mesh for 360 degree attraction rate.- Full protective outer mesh for high safety use.- Large collection tray for easy cleaning.- Can be free standing or hanging.- Country of origin China | **1** |  |  |
| **Dishwashing Area** |  |  |  |
| 1 | **S/S SORTING TABLE WITH BACK SPLASH, WITH TRASH HOLE , DIM.:240x70x90 CM**- Body entirely made of Stainless Steel AISI 304.- Work top made of 1.5mm polished Stainless Steel and reinforced by stainless steel U-shaped channels with polyurethane tapes acting as sound deadening pads.- Frame work made of 40x40mm Stainless Steel square tubes thickness of1.2mm, all joints on the table structure fixed by welding.- Stainless Steel height adjustable feet. Technical Features: Dimensions (mm) : 2400 W x 700 D x 900 H | **1** |  |  |
| 2 | **KARMA-JIWINS PLASTIC WASTE BIN WITH LID MODEL OT120-101,** CAP.: 75.7 Ltr. | **1** |  |  |
| 3 | **WALL MOUNTED RACK SHELF DIM : 110x55 CM** **-** Body entirely made of Stainless Steel AISI 304.- Shelf provided with Drain hole- capacity : 2 dishwasher rackes 50x50 cm (price do not includ racks) | **1** |  |  |
| 4 | **INLET TABLE WITH DOUBLE BOWL SINK UNIT WITHOUTLOWER**SHELF : 190X70X90 CM | **1** |  |  |
| 4.1 | **(Accessory) DOUBLE SIPHON** | **1** |  |  |
| 4.2 | **(Accessory) PRE-WASH SPRAY UNIT** | **1** |  |  |
| 5 | **OUTLET TABLE, 60 CM** - Body entirely made of Stainless Steel AISI 304.- Work top made of 1.5 mm polished Stainless Steel.- Frame work made of 40x40mm Stainless Steel square tubes thickness of 1.2mm, all joints on the table structure fixed by welding.- Stainless Steel height adjustable feet.- Country of Origin: JORDAN Technical Features: Dimensions (mm) : 600 W x 600 D x 900 H | **1** |  |  |
| 6 | **PERFORATED SHELVING UNIT, 170 CM** - Body entirely made of Stainless Steel AISI 304.- Shelving unit is provided with four perforated fixed by screw and nuts shelves.- Shelving unit is mounted on four angle posts 1.5mm thickness.- Maximum load per shelf (with evenly distributed weight): 150Kg.- Shelving unit is provided with height adjustable feet.Technical Features:Dimensions (mm) : 1700 W x 500 D x 1800 H | **2** |  |  |
| **Storage Area** |  |  |  |
| 1 | **PAINTED STEEL SIDE UPRIGHT, DIM.: 40x200 CM** **-** Side upright consists of 2 columns made of powder coated steel with thickness 1.5 mm and 3 cm cross section.- Columns are connected together with special steel plate. | **11** |  |  |
| 2 | **PAINTED STEEL SHELF, DIM.: 97x40CM** - Shelves thickness 0.8 mm.- Shelves load 80 kg distributed on each shelf.- Shelves can be adjustable in highest without using any tools.- Shelves are powder coated. | **40** |  |  |