1- Item: HP Color LaserJet Enterprise M553D duplex

|  |  |
| --- | --- |
| Offered equipment is in full conformity with the below technical specifications | Documentation attached to your submission  (Yes / No)  and additional comments from bidder \* |
|  Functionality: Print-only, color laser printer   Print Speed: Up to 40 pages per minute (ppm) for both black and color   First Page Out Time: As fast as 6 seconds (black), 7 seconds (color)   Print Resolution: Up to 1200 x 1200 dpi   Duplex Printing: Automatic two-sided printing   Monthly Duty Cycle: Up to 80,000 pages   Recommended Monthly Page Volume: 2,000 to 6,000 pages   Processor: 1.2 GHz   Memory: Standard 1 GB, expandable to 2 GB   Storage: 4 GB non-volatile memory   Paper Handling:   * Standard Input Capacity: 650 sheets (100-sheet multipurpose tray, 550-sheet input tray) * Maximum Input Capacity: Up to 2,300 sheets with optional trays * Output Capacity: 250 sheets * Supported Media Sizes: 3 x 5 inches to 8.5 x 14 inches * Supported Media Types: Plain, light, bond, recycled, mid-weight, heavy, mid-weight glossy, heavy glossy, extra heavy, extra heavy glossy, cardstock, card glossy, color transparency, labels, letterhead, envelopes, preprinted, prepunched, colored, rough, opaque film, user-defined    Connectivity:   * Standard Interfaces: Hi-Speed USB 2.0, Gigabit Ethernet 10/100/1000Base-TX   + 1 additional complete sets of toners  One year warrant | Please confirm if the offered specificaiton match with the tendered specification (Yes / No), if not, please type here the offered specification |
| Warranty Period | One Year |

2- Item: **ARTronic 3kVA Online UPS**

|  |  |
| --- | --- |
| Offered equipment is in full conformity with the below technical specifications | Documentation attached to your submission  (Yes / No)  and additional comments from bidder \* |
|  Power Capacity: 3000 VA   Technology: True double-conversion online UPS   Power Factor: 0.7 to 0.9   Input Voltage Range: 110–300 VAC (single-phase)   Output Voltage: 220 VAC ±1%   Frequency: 50 Hz ±0.2% (battery mode)   Voltage Waveform: Pure sine wave   Total Harmonic Distortion (THD): ≤3%   Overload Capacity: 10 minutes at 105–130% load; immediate transfer to bypass above 130%   Short Circuit Protection: Electronic protection with automatic inverter shutdown   Transfer Time: 0 ms (line to battery), typical 2.5 ms (inverter to bypass)   Battery Configuration: 8 × 12V 7Ah or 9Ah sealed lead-acid batteries   Backup Time: Approximately 6 minutes at full load   Recharge Time: 5 hours to 90% capacity   Display: LCD or LED panel (model-dependent)   Communication Ports: RS-232, USB; optional SNMP slot   Software Compatibility: Windows, Linux, Novell   Operating Temperature: 0°C to 40°C   Humidity: 0–90% RH (non-condensing)   Noise Level: <50 dBA | Please confirm if the offered specificaiton match with the tendered specification (Yes / No), if not, please type here the offered specification |
| Warranty Period | One Year |

3- Item: Hikvision EKI-K41T44 4-Channel 4K NVR with 4 x 4MP Night Vision Turret Cameras

|  |  |
| --- | --- |
| Offered equipment is in full conformity with the below technical specifications | Documentation attached to your submission  (Yes / No)  and additional comments from bidder \* |
|  Resolution: Each camera captures 4MP (2560 × 1440) video at 20 fps. 4 cameras included   Night Vision: Infrared night vision up to 65 feet.   NVR: 4-channel 8MP NVR with 1TB preinstalled HDD; supports up to 6TB.   Video Compression: H.265+/H.265/H.264+/H.264/MPEG-4.   Outdoor Use: Cameras are IP67-rated for weather resistance.   Field of View: 2.8mm fixed lens providing a 100° horizontal field of view. | Please confirm if the offered specificaiton match with the tendered specification (Yes / No), if not, please type here the offered specification |
| Warranty Period | One Year |

4- Item: UPS Batteries

|  |  |
| --- | --- |
| Offered equipment is in full conformity with the below technical specifications | Documentation attached to your submission  (Yes / No)  and additional comments from bidder \* |
| Type: Sealed Lead Acid (SLA) Battery  Nominal Voltage: 12V  Rated Capacity: 9Ah  Battery Terminals: F2 Terminals  Dimensions (L x W x H): 5.95 x 2.56 x 3.86 inches (151 x 65 x 98 mm)  Weight: Approximately 5.6 lbs (2.54 kg)  Operating Temperature: Discharge: -20°C to 60°C (-4°F to 140°F)  Charge: -20°C to 50°C (-4°F to 122°F)  Storage: -20°C to 50°C (-4°F to 122°F)  Life Expectancy: 3-5 years. | Please confirm if the offered specificaiton match with the tendered specification (Yes / No), if not, please type here the offered specification |
| Warranty Period | One Year |

5- Item: Samsung 55 Inch LED TV 4K

|  |  |
| --- | --- |
| Offered equipment is in full conformity with the below technical specifications | Documentation attached to your submission  (Yes / No)  and additional comments from bidder \* |
| Samsung 55 Inch LED TV standard, 4K | Please confirm if the offered specificaiton match with the tendered specification (Yes / No), if not, please type here the offered specification |
| Warranty Period | One Year |

6- Item: Solar Lamps big size

|  |  |
| --- | --- |
| Offered equipment is in full conformity with the below technical specifications | Documentation attached to your submission  (Yes / No)  and additional comments from bidder \* |
| Guiding specs, not binding  اللوحة الشمسية/ 20W 6V  البطارية/ ليثيوم 15000Mah 3.2v  قوة الإضاءة/ 1350 لومن  مساحة تغطية الإضاءة/ 100m مربع .  مدة الشحن/ 8 ساعات تحت أشعة الشمس المباشرة.  المقاسات/ 63cm\*25cm\*5cm  كشاف شارع بالطاقة الشمسية 90 واط 1350 لومن | Please confirm if the offered specificaiton match with the tendered specification (Yes / No), if not, please type here the offered specification |
| Warranty Period | One Year |

7- Item: spotlights/flashlights

|  |  |
| --- | --- |
| Offered equipment is in full conformity with the below technical specifications | Documentation attached to your submission  (Yes / No)  and additional comments from bidder \* |
| Rechargeable spotlights/flashlights | Please confirm if the offered specificaiton match with the tendered specification (Yes / No), if not, please type here the offered specification |
| Warranty Period | One Year |

8- Item: USB to Ethernet adapter

|  |  |
| --- | --- |
| Offered equipment is in full conformity with the below technical specifications | Documentation attached to your submission  (Yes / No)  and additional comments from bidder \* |
| USB to Ethernet Adapter 10/100 speed, usb3.0 | Please confirm if the offered specificaiton match with the tendered specification (Yes / No), if not, please type here the offered specification |
| Warranty Period | One Year |

9- Item: Water Dispenser – Generic Model with Hot & Cold Taps

|  |  |
| --- | --- |
| Offered equipment is in full conformity with the below technical specifications | Documentation attached to your submission  (Yes / No)  and additional comments from bidder \* |
|  Type: Floor-standing or tabletop (varies by model)   Functions: Cold water, hot water, ambient water (optional)   Cooling Method: Compressor-based or electronic (thermoelectric)   Hot Water Temperature: 85°C to 95°C   Cold Water Temperature: 5°C to 10°C   Heating Power: 500W – 750W   Cooling Power: 65W – 120W   Water Output Capacity:   * Hot: 4 – 5 liters/hour * Cold: 2 – 3 liters/hour   One year warranty | Please confirm if the offered specificaiton match with the tendered specification (Yes / No), if not, please type here the offered specification |
| Warranty Period | One Year |

10- Item: Generic USB Keyboard

|  |  |
| --- | --- |
| Offered equipment is in full conformity with the below technical specifications | Documentation attached to your submission  (Yes / No)  and additional comments from bidder \* |
| USB Keyboard, with Arabic keys | Please confirm if the offered specificaiton match with the tendered specification (Yes / No), if not, please type here the offered specification |
| Warranty Period | One Year |

11- Item: Generic USB Mouse

|  |  |
| --- | --- |
| Offered equipment is in full conformity with the below technical specifications | Documentation attached to your submission  (Yes / No)  and additional comments from bidder \* |
| USB Mouse, optical | Please confirm if the offered specificaiton match with the tendered specification (Yes / No), if not, please type here the offered specification |
| Warranty Period | One Year |